 Reads commands from Serial without blocking rest of the program
 Commands terminated by <space> , CR or NL
 The Arduino monitor must be set to Newline or Carrage Return or Both NL & CR for this sketch to work.